



**Manhole Inspection Checklist**


Manhole Number: \_\_\_\_\_\_\_\_\_\_\_ Inspector: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Manhole Barrier Diameter: \_\_\_\_\_\_\_\_\_\_\_ Interceptor: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Manhole Depth (Rim to Invert):\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**This model form/template must be customized to meet your Agency’s needs.**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Item Inspected** | **Date Inspected**  (date each line that applies) | | | **Repairs Needed**  (√ each that applies) | | | **Repairs Made** | **Date Repairs Made** | |
| COVER | Lift Pin | / / | | Needs Pin | |  |  | / / |
|  | Bolt Down | / / | | Bolt Missing | |  |  | / / |
|  | Locking | / / | | Replace | |  |  | / / |
|  | Non-Rocking | / / | |  | |  |  |  |
| CASTING | Badly Rusted | / / | | Reset | |  |  | / / |
|  | Knocked Loose | / / | | Raise | |  |  | / / |
|  | Good Condition | / / | | Replace | |  |  | / / |
| CHIMNEY | Brick | / / | | Leaks | |  |  | / / |
|  | Concrete | / / | | Re-mortar | |  |  | / / |
|  | Good Condition | / / | | Replace | |  |  | / / |
|  | Loose Mortar | / / | |  | |  |  | / / |
|  | Offset Opening | / / | |  | |  |  | / / |
|  | Center Opening | / / | |  | |  |  | / / |
| BARRELS | Good Condition | / / | | Leaks | |  |  | / / |
|  | Slight Corrosion | / / | |  | |  |  | / / |
|  | Bad Corrosion | / / | |  | |  |  | / / |
| BENCH | Grease Build-up | / / | | Clean | |  |  | / / |
|  | Bad Concrete | / / | | Patch | |  |  | / / |
|  | Good Condition | / / | |  | |  |  | / / |
| CHANNEL | Rocks in Channel | / / | | Clean | |  |  | / / |
|  | Grease Build-up | / / | |  | |  |  | / / |
|  | Bad Corrosion | / / | |  | |  |  | / / |
|  | Depth of Flow | / / | |  | |  |  | / / |
|  | Depth of Grit | / / | |  | |  |  | / / |
| INTER- | CHECK | YES | NO | Leaks |  | |  | | | |
| CEPTER | Lamped |  |  |  |  | | Incoming Lines: | | | |
|  | Loose Gaskets |  |  |  |  | | Sketch location, note size, | | | |
|  | Infiltration |  |  |  |  | | and measure height | | | |
|  | Slight Corrosion |  |  |  |  | | of all incoming lines | | | |
|  | Bad Corrosion |  |  |  |  | | (from the pipe invert.) | | | |
|  | Scratch Test |  |  |  |  | |  | | | |
|  | Scratch Depth |  | Inches |  |  | |  | | | |

****

|  |  |
| --- | --- |
| Additional Comments / Observations: |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |